Open topic with navigation

# Video Server Analysis Task Parameters

Deprecated: This task is deprecated in HPE Connector Framework Server version 11.1.0 and later. It is still available for existing implementations, but it might be incompatible with new functionality. The task might be removed in future.

HPE recommends using the MediaServerAnalysis task instead.

The parameters in this section customize the `VideoServerAnalysis` task.

This task runs analysis on videos that are associated with documents and have the field `AUTN_NEEDS_VIDEO_SERVER_ANALYSIS`. You must add this field to the documents that you want to analyze. You can add the field using a Lua script.

You can run the `VideoServerAnalysis` task as a Pre or Post task. When you configure the task, use the `Pre` or `Post` parameter to specify the name of a section in the HPE CFS configuration file that contains the task settings:

    [ImportTasks]
    Post0=Lua:DetectVideos.lua
    Post1=VideoServerAnalysis:VideoServerSettings

    [VideoServerSettings]
    VideoServerHost=server:14000,server2:14000
    VideoServerConfigurationName=broadcast
    VideoAnalysisTransform=xslt/VideoServerAnalysisTransform.xsl

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm