Open topic with navigation

# MaxFileUploadSize

The `MaxFileUploadSize` parameter specifies the maximum amount of data (in bytes) accepted by the server through an HTTP POST request. This parameter therefore limits the amount of data that can be sent to the server in an ACI action. To specify an unlimited size, set this parameter to `-1`.

Note: The default configuration for Connector Framework Server sets this parameter to `-1`. HPE recommends that you do not change the value of this parameter.

Type: | Long
Default: | `10000000`
Required: | No
Configuration Section: | Server
Example: | `MaxFileUploadSize=-1`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm