Open topic with navigation

# ACIThreadStatus

Returns information about the activity of all the threads that the ACI service is using, including the number of accepted connections.

Note: This is a status action that can be sent only from ServiceStatusClients (which are set in the `[Service]` section of the configuration file).

## Example

    http://12.3.4.56:9002/action=ACIThreadStatus

This action uses port 9002 to request the status of all the threads that the service is using. The service is located on a machine with the IP address 12.3.4.56.

## Parameters

None

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm