Open topic with navigation

# ScheduleRepeatSecs

The `ScheduleRepeatSecs` parameter specifies the interval (in seconds) from the start of one scheduled `synchronize` cycle to the start of the next. If a previous synchronize cycle is still running when the interval elapses, the connector queues a maximum of one action.

This parameter has an effect only if the `EnableScheduledTasks` parameter is set to `True`.

Type: | Integer
Default: | 1
Required: | No
Configuration Section: | TaskName or FetchTasks or Connector
Example: | `ScheduleRepeatSecs=3600`
See Also: | EnableScheduledTasks ScheduleCycles ScheduleStartTime

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm