Open topic with navigation

# PerfMonQueryFrequency

The amount of time, in seconds, that the connector waits between taking readings from a performance counter.

Note: Performance monitoring is supported on Windows platforms only.

Type: | Integer
Default: | 5
Recommended Range: | Minimum: 1 Maximum: 10
Required: | No
Configuration Section: | TaskName or FetchTasks
Example: | `PerfMonQueryFrequency=10`
See Also: | PerfMonAvgOverReadings PerfMonCounterMaxN PerfMonCounterMinN PerfMonCounterNameN

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm