Open topic with navigation

# MaxGlobalKBPS

The maximum bandwidth the connector can use to download Web pages. Specify a value in kilobytes per second. If you do not want to restrict the bandwidth, enter 2000000000.

Type: | Long
Default: | 8192
Required: | No
Allowed Range: | Minimum: 1 Maximum: 2000000000
Recommended Range: | Minimum: 8 Maximum: 2048
Configuration Section: | TaskName or Default
Example: | `MaxGlobalKBPS=512`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm