Open topic with navigation

# IngestConfigSection

The `IngestConfigSection` parameter specifies the name of a section in the connector’s configuration file that contains the ingestion settings.

You can use this parameter to override the `[Ingestion]` section and send data to a different CFS or to a connector for one particular task.

Type: | String
Default: | TaskName
Required: | No
Configuration Section: | TaskName
Example: | `IngestConfigSection=MyTask1`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm