Open topic with navigation

# ACI Encryption Configuration Parameters

You can encrypt communications between ACI servers (for example, HPE Community Component and License Server) and any applications that use the HPE ACI API by configuring an `[ACIEncryption]` section in each of the application configuration files.

Note: Instead of using ACI encryption, HPE recommends configuring Secure Socket Layer (SSL) connections between ACI servers and applications. For more information, see Secure Socket Layer Parameters.

For example:

    [ACIEncryption]
    CommsEncryptionType=GSS
    ServiceName=Kerberos

CommsAllowUnencrypted

CommsEncryptionType

ServiceName

See Also: Secure Socket Layer Parameters.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm