Open topic with navigation

# SocketTimeout

The number of seconds to timeout for index actions sent to the HPE Content Component index port.

Type: | Long
Default: | 60
Required: | No
Configuration Section: | IndexServer
Example: | `SocketTimeout=90`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm