Open topic with navigation

# N

The names of the flush lock server configuration sections.

For the name of this configuration parameter, replace `N` with the zero-based rank number of the specified field process. For the parameter value, type the name of the lock server configuration section.

Note: You must number the lock server parameters in consecutive order starting from 0 (zero).

Type: | Integer
Default: |
Required: | No
Configuration Section: | FlushLock
Example: | `0=LockServer1 1=LockServer2 2=LockServer3`
See Also: | Lock Server Configuration Parameters

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm