Open topic with navigation

# BackupInterval

The time between backups. Specify the time in the 24-hour clock, in the format `hh:mm`.

When you start HPE Content Component, the specified `BackupInterval` must elapse (after the specified BackupTime) before the first backup takes place.

To run daily backups, set `BackupInterval` to `0`.

Type: | Long
Default: | 0
Required: | No
Configuration Section: | Schedule
Example: |
    BackupInterval=12:00
    BackupTime=19:00
In this example, if you start HPE Content Component at 18:00, the first backup occurs at 07:00 the following day.
See Also: | Backup BackupCompression BackupDirN BackupMaintainDirStructure BackupRetryAttempts BackupRetryPause BackupTime NumberOfBackups

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm