Open topic with navigation

# Threads

The maximum number of parallel actions that HPE Controller can process at any one time. The optimum number of threads is generally the number of CPUs plus one spare thread.

Type: | Long
Default: | 10
Allowed Range: | Minimum: 1 Maximum: 32
Recommended Range: | Minimum: 4 Maximum: 32
Required: | No
Configuration Section: | Server
Example: | `Threads=2`
See Also: |

© 2013 - 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm