Open topic with navigation

# StrictMode

Whether to receive messages indicating that at least one child server responds or at least one child server does not respond.

Distributed Action Handler returns error descriptions in its error response when in `StrictMode`, and writes the descriptions to the action log. These error descriptions can come from child servers.

`0` | Distributed Action Handler returns a successful response when at least one child server returns a success response.
`1` | Distributed Action Handler returns an error response if at least one child server does not return a success response. Use this option if results from all child servers are critical.
`2` | Distributed Action Handler returns an error response if at least one child server fails to respond. It is otherwise equivalent to mode 0.

Type: | Long
Default: | 0
Required: | No
Configuration Section: | Server
Example: | `StrictMode=1`
See Also: | Secure Socket Layer Parameters

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close We welcome your comments! To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm