Open topic with navigation

# Distributed Engine Configuration Parameters

If you install and operate the HPE Distributed Action Handler as a Standalone component, you must create a `[DistributedEngine` `N``]` section for each of the IDOL servers or other child servers that the HPE Distributed Action Handler communicates with, in which you can specify the server configuration details. See Child Server Configuration Parameters.

Note: You must set the DistributedEngines parameter in the `[Server]` section to the number of distribution child servers you create.

For example:

    [DistributedEngine0]
    Host=testserver1
    Port=9000
    Type=IDOL

    [DistributedEngine1]
    Host=testserver2
    Port=9920
    Type=K2

    [DistributedEngine2]
    Host=testserver3
    Port=210
    Type=Z39.50
    DefaultRelevance=80
    RequiresAuthentication=TRUE
    QueryFormat=PQF
    ResponseFormat=XML

Note: This configuration for the HPE Distributed Action Handler distribution child servers is not used for IDOL integrated HPE Distributed Action Handler.

- For integrated configurations in which HPE Distributed Action Handler and DIH are configured together, see Distribution IDOL Servers Configuration Parameters.
- For integrated configurations in which HPE Distributed Action Handler and DIH are configured separately, see HPE Distributed Action HandlerEngines Configuration Parameters.

DefaultRelevance

Host

HostPortAlias

Krb5Realm

Krb5Service

MirrorName

MSWindows

Name

Port

Priority

QueryFormat

QueryURI

RequiresAuthentication

ResponseFormat

SecurityKeys

SecurityType

SSLConfig

Type

Weight

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm