Open topic with navigation

# PingTimeout

The number of seconds that must elapse before the HPE Distributed Action Handler times out `GetStatus` requests to the child servers.

Type: | Long
Default: | 1
Allowed Range: | Minimum: 1 Maximum: 60
Recommended Range: | Minimum: 1 Maximum: 10
Required: | No
Configuration Section: | Server
Example: | `PingTimeout=3`
See Also: | EngineTimeout

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm