Open topic with navigation

# DistributedCommands

The number of distributed commands that you want to configure. Distributed commands are only applicable in mirror mode. They are actions that are distributed to all child servers. The response returned by the child servers is merged using the associated XSL template.

For each action you must create a `[DistributedCommandN]` configuration section.

Type: | Long
Default: | 0
Allowed Range: | Minimum: 0 Maximum: 32767
Required: | No
Configuration Section: | Server
Example: | `DistributedCommands=5`
See Also: | Distributed Command Configuration Parameters

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm