Open topic with navigation

# Port

The port that HPE DAH uses to send actions to the child server.

If you create a server group by specifying a comma-separated list of host names in the Host parameter, you must specify a value in the `Port` parameter for each mirrored child server.

Type: | Long
Default: | -1
Allowed Range: | Minimum: 1 Maximum: 65535
Recommended Range: | Minimum: 1025 Maximum: 65535
Required: | Yes
Configuration Section: | IDOLServer `N` or DistributedEngine `N` or DAHEngine `N`
Example: | `Port=9000`
See Also: | Host Type Weight

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm