Open topic with navigation

# RequiredParams

The number of parameters that are required for HPE Distributed Action Handler to send the action to all the child servers.

You must define a ParamNameN and ParamValueN for each required parameter.

Note: You must number the parameters in consecutive order, starting from 0 (zero).

Type: | String
Default: |
Required: | No
Configuration Section: | DistributedCommand `N`
Example: | `RequiredParams=2`
See Also: | ParamNameN ParamValueN

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm