Open topic with navigation

# EngineTimeout

The number of seconds after which the HPE Distributed Action Handler connection to a child server times out if the HPE Distributed Action Handler does not receive a reply.

Type: | Long
Default: | 60
Allowed Range: | Minimum: 1 Maximum: 86400
Recommended Range: | Minimum: 1 Maximum: 600
Required: | No
Configuration Section: | Server
Example: | `EngineTimeout=60`
See Also: | EngineMaxRetries MaxVDBEngines PingTimeout

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm