Open topic with navigation

# DAHEngine`N` Configuration

In the `[DAHEngines]` section you must create a `[DAHEngineN]` subsection for each IDOL server to which the HPE Distributed Action Handler sends actions. Each `[DAHEngineN]` subsection specifies the host and ACI port of a child IDOL server. See Child Server Configuration Parameters.

Note: You must number child IDOL server sections in consecutive order, starting from 0 (zero).

For example:

    [DAHEngines]
    Number=2

    [DAHEngine0]
    Host=localhost
    Port=9000

    [DAHEngine1]
    Host=12.3.4.56
    Port=9000

DefaultRelevance

Host

HostPortAlias

Krb5Realm

Krb5Service

MirrorName

MSWindows

Name

Port

Priority

QueryFormat

QueryURI

RequiresAuthentication

ResponseFormat

SecurityKeys

SecurityType

SSLConfig

Type

Weight

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm