Open topic with navigation

# HPE Distributed Action HandlerEngines Configuration Parameters

If you install and operate the HPE Distributed Action Handler as integrated with IDOL, you can configure child engines for HPE Distributed Action Handler and DIH separately. This option allows you increased flexibility when querying and indexing content in remote servers. For example, you might define multiple DIH child engines for content that you index through a combination of failover and mirroring.

Use the `[DAHEngines]` section to set the total number of IDOL servers to which the HPE Distributed Action Handler sends actions.

You must create a `[DAHEngineN]` subsection for each child engines that HPE Distributed Action Handler must send actions to. In this section, you specify the child server configuration details.

For example:

    [DAHEngines]
    Number=2

    [DAHEngine0]
    Host=localhost
    Port=9000

    [DAHEngine1]
    Host=12.3.4.56
    Port=9000

Note: This configuration for the HPE Distributed Action Handler distribution child servers is not used for Standalone HPE Distributed Action Handler.

- For Standalone configuration see Distributed Engine Configuration Parameters
- For Integrated configuration in which HPE Distributed Action Handler and DIH are configured together, see Distribution IDOL Servers Configuration Parameters

Number

DAHEngineN

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm