Open topic with navigation

# CommsEncryptionType

Encryption type for returned data.

Note: Instead of using ACI encryption, HPE recommends configuring Secure Socket Layer (SSL) connections between ACI servers and applications. For more information, see Secure Socket Layer Parameters.

Use one of the following values:

- `GSS`. Use this option if HPE Distributed Action Handler is part of a system that is using Kerberos protocol for communication.

  To use this option, you must have a suitable library to provide the GSSAPI. On Linux systems, you might also need to create a symbolic link for the GSSAPI library to `gssapi32.so` in the working directory of the component.

Type: | String
Default: |
Required: | No
Configuration Section: | ACIEncryption
Example: | `CommsEncryptionType=GSS`
See Also: | CommsAllowUnencrypted ServiceName

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm