Open topic with navigation

# Manage Client Connections

You can control several aspects relating to clients connecting to the HPE DIH. Use the following configuration parameters, which you set in the `[Server]` section of the HPE DIH configuration file.

`IndexClients` | The host machines that have permission to send index actions to HPE DIH. Set this to one or more host names or IP addresses. You can use Wildcard values.
`RecvTimeout` | How long the HPE DIH attempts to read an client index action before it times out. The default value is 60 seconds. A small value can improve the indexing speed, but might drop more actions.
`RecvDuration` | How long a communication between the HPE DIH and a client can last (in either direction). The default value is 600 seconds. A large value allows you to index more data with each action.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm