Open topic with navigation

# SSLConfig

Identifies the configuration section in which the SSL configuration details for distributed servers are specified, usually `SSLOptionN`. This option allows SSL connections between the HPE Distributed Index Handler and other components.

Set this parameter in the `[Server]` section of the HPE Distributed Index Handler configuration file to configure SSL for incoming ACI calls.

Additionally, to configure SSL for the incoming calls to the HPE Distributed Index Handler index port, set SSLConfig in the `[IndexServer]` section. For outgoing ACI calls, set SSLConfig in the `[IDOLServerN]` or `[DIHEngineN]` section.

Note: To define one set of SSL options that are shared by multiple communications, define only one `SSLOption` section. Set the `SSLConfig` parameters in each section to the single `SSLOption` section.

Type: | String
Default: |
Required: | No
Configuration Section: | Server or other section for outgoing communications
Example: | `SSLConfig=SSLOption0`
See Also: | Secure Socket Layer Parameters

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm