Open topic with navigation

# Troubleshooting

This section describes some common issues and their solutions. If your HPE DIH is not functioning correctly, try the remedies described in this appendix.

- The HPE DIH cannot obtain a valid service port

  If the HPE DIH cannot obtain a valid service port, it displays the following warning:

      Warning: Engine n. Unable to obtain a valid service port.

  To resolve this issue, verify that:

  - the HPE DIH IP address has been correctly added to the `QueryClient` setting in the IDOL Server configuration files.

  - the IDOL Servers are all version 4.5.0. or later.

- Actions fail

  If the ACI actions that you send to the HPE DIH fail, verify that:

  - the HPE DIH IP address has been correctly added to the `QueryClients` setting in the IDOL Server configuration files.
  - the HPE DIH IP address has been correctly added to the `ServiceStatusClients` setting in the IDOL Server configuration files.

- Index actions fail

  If the index actions that you send to the HPE DIH fail, verify that the HPE DIH IP address has been correctly added to the `IndexClients` setting in the IDOL Server configuration files.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm