Open topic with navigation

# RecvDuration

The number of seconds that communications to and from the HPE Distributed Index Handler are permitted to last.

Type: | Integer
Default: | 600
Required: | No
Configuration Section: | Server
Example: | `RecvDuration=900`
See Also: | RecvTimeout

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm