Open topic with navigation

# Determine the State of Child Servers

The HPE DIH regularly pings all its child IDOL servers to determine their state; running (up) or not running (down). In mirror mode, if a server is down, the HPE DIH queues the data for that server, and indexes the data into the server when it is available again. In non-mirror mode, the HPE DIH redistributes the data among the available servers. In this case, it also queues any updates to documents that have already been indexed, and sends the updates when the server is available again.

You can configure how often the HPE DIH checks the state of its child servers. Set the `PingInterval` parameter in the `[Server]` section of the HPE DIH configuration file to the time interval between checks. The default value is 20 seconds.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm