Open topic with navigation

# UserClients

The IP addresses for machines that are permitted to send actions to the Port.

Separate multiple addresses with commas. There must be no space before or after a comma.

Type: | String
Default: | *
Required: | No
Configuration Section: | Server
Example: | `UserClients=12.34.56.7,2.4.6.8`
See Also: | Port ProxyClients

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm