Open topic with navigation

# Install HPE IDOL on UNIX

Use the following procedure to install HPE IDOL in text mode on UNIX platforms.

To install HPE IDOL on UNIX

1. Open a terminal in the directory in which you have placed the installer, and enter the following command:

       ./IDOLServer_VersionNumber_Platform.exe --mode text

   where:

   `VersionNumber` | is the product version
   `Platform` | is the name of your UNIX platform

   Note: Ensure that you have execute permission for the installer file.

   The console installer starts and displays the Welcome screen.

2. Read the information and then press the `Enter` key.

   The license information is displayed.

3. Read the license information, pressing `Enter` to continue through the text. After you finish reading the text, type `Y` to accept the license terms.

4. Type the path to the location where you want to install the servers, or press `Enter` to accept the default path.

   The Installation Mode screen is displayed.

5. Press `2` to select the Custom installation mode.

   The License Server screen opens. Choose whether you have an existing License Server.

   - To use an existing License Server, type `Y`. Specify the host and port details for your License Server (or press ``Enter`` to accept the defaults), and then press `Enter`. Go to Step 7.
   - To install a new instance of License Server, type `N`.

6. If you want to install a new License Server, provide information for the ports that the License Server uses.

   1. Type the value for the ACI Port and press `Enter` (or press `Enter` to accept the default value).

      ACI Port | The port that client machines use to send ACI actions to the License Server.

   2. Type the value for the Service Port and press `Enter` (or press `Enter` to accept the default value).

      Service Port | The port by which you send service actions to the License Server. This port must not be used by any other service.

   3. Type the location of your HPE license key file (`licensekey.dat`), which you obtained when you purchased HPE IDOL. Press `Enter`.

7. The Component Selection screen is displayed. Press `Enter`. When prompted, type `Y` for the components that you want to install. Specify the port information for each component, and then press `Enter`. Alternatively, leave the fields blank and press `Enter` to accept the default port settings.

   For each component, you can optionally provide port information to specify the ports that the component must use. The port that you choose must not be used by any other service. The installer allows you to set the following port types:

   ACI Port | The port that client machines use to send ACI actions to the component.
   Index Port | The port that client machines use to send index actions to the component. This port is available only for the Content, Agentstore, and DIH components.
   Service Port | The port that client machines use to send service requests to the component. This port is also the port that the component uses for License Server communication.
   Binary Data Port | The port to use for streaming audio data. This port is available only for the IDOL Speech Server component.

   The following table lists the components and subcomponents that you can install, and the default port that the installer uses if you do not provide an alternative value. You must change the port information if the default port value is already in use.

   Component | Default port information
   --- | ---
   Content | ACI Port: 9100 Index Port: 9101 Service Port: 9102
   Agentstore | ACI Port: 9050 Index Port: 9051 Service Port: 9052
   Category | ACI Port: 9020 Service Port: 9022
   Community | ACI Port: 9030 Service Port: 9032
   View | ACI Port: 9080 Service Port: 9082
   QMS | ACI Port: 16000 Service Port: 16002
   QMS subcomponent: Statistics Server | ACI Port: 19870 Service Port: 19872
   Controller | ACI Port: 41200 Service Port: 41202
   Coordinator | ACI Port: 40200 Service Port: 40202
   DAH | ACI Port: 9060 Service Port: 9062
   DIH | ACI Port: 9070 Index Port: 9071 Service Port: 9072
   CFS | ACI Port: 7000 Service Port: 17000
   File System Connector | ACI Port: 7002 Service Port: 17002
   Web Connector (Linux) | ACI Port: 7006 Service Port: 17006
   HTTP Connector (Solaris) | ACI Port: 7004 Service Port: 17004
   Media Server | ACI Port: 14000 Service Port: 14001
   Speech Server | ACI Port: 15000 Service Port: 15001 Binary Data Port: 15002
   Knowledge Graph | ACI Port: 10300 Service Port: 10302
   Find | HTTP Port: 8080
   BIFHI | HTTP Port: 8080

   For more information about these components, see IDOL Core Components.

   Note: These ports must not be used by any other service.

   The Init Scripts screen is displayed.

8. Type the user that the server should run as, and then press `Enter`.

   Note: The installer does not create this user. It must exist already.

9. Type the group that the server should run under, and then press `Enter`.

   Note: If you do not want to generate init scripts for installed components, you can simply press `Enter` to move to the next stage of the installation process without specifying a user or group.

   The Summary screen is displayed.

10. Verify the settings that you made, then press `Enter` to begin installation.

    The Installing screen is displayed.

    This screen indicates the progress of the installation process.

    The Installation Complete screen is displayed.

11. Press `Enter` to finish the installation.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm