Open topic with navigation

# SleepBetweenSentEmails

The length of time (in milliseconds) that the HPE IDOL Server mailing operation must wait after it has sent a batch of e-mails before it sends another batch.

Type: | Long
Default: | 0
Required: | No
Configuration Section: | `MyCustomFunctionality`
Example: | `SleepBetweenSentEmails=50`
See Also: | MaxEmailsToSendBatchProcess RunMailer

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm