Open topic with navigation

# Install HPE Media Server on UNIX

Use the following procedure to install HPE Media Server in text mode on UNIX platforms.

To install HPE Media Server on UNIX

1. Open a terminal in the directory in which you have placed the installer, and enter the following command:

       ./IDOLServer_VersionNumber_Platform.exe --mode text

   where:

   `VersionNumber` | is the product version
   `Platform` | is the name of your UNIX platform

   Note: Ensure that you have execute permission for the installer file.

   The console installer starts and displays the Welcome screen.

2. Read the information and then press the `Enter` key.

   The license information is displayed.

3. Read the license information, pressing `Enter` to continue through the text. After you finish reading the text, type `Y` to accept the license terms.

4. Type the path to the location where you want to install the servers, or press `Enter` to accept the default path.

   The Installation Mode screen is displayed.

5. Press `2` to select the Custom installation mode.

   The License Server screen opens. Choose whether you have an existing License Server.

   - To use an existing License Server, type `Y`. Specify the host and port details for your License Server (or press ``Enter`` to accept the defaults), and then press `Enter`. Go to Step 7.
   - To install a new instance of License Server, type `N`.

6. If you want to install a new License Server, provide information for the ports that the License Server uses.

   1. Type the value for the ACI Port and press `Enter` (or press `Enter` to accept the default value).

      ACI Port | The port that client machines use to send ACI actions to the License Server.

   2. Type the value for the Service Port and press `Enter` (or press `Enter` to accept the default value).

      Service Port | The port by which you send service actions to the License Server. This port must not be used by any other service.

   3. Type the location of your HPE license key file (`licensekey.dat`), which you obtained when you purchased HPE Media Server. Press `Enter`.

7. The Component Selection screen is displayed. Press `Enter`. When prompted, type `Y` for the components that you want to install. Specify the port information for each component, and then press `Enter`. Alternatively, leave the fields blank and press `Enter` to accept the default port settings.

   For HPE Media Server you must specify the following information:

   ACI Port | The port that you want HPE Media Server to listen on, for ACI actions.
   Service Port | The port that you want HPE Media Server to listen on, for service actions.

   Note: These ports must not be used by any other service.

   The Init Scripts screen is displayed.

8. Type the user that the server should run as, and then press `Enter`.

   Note: The installer does not create this user. It must exist already.

9. Type the group that the server should run under, and then press `Enter`.

   Note: If you do not want to generate init scripts for installed components, you can simply press `Enter` to move to the next stage of the installation process without specifying a user or group.

   The Summary screen is displayed.

10. Verify the settings that you made, then press `Enter` to begin installation.

    The Installing screen is displayed.

    This screen indicates the progress of the installation process.

    The Installation Complete screen is displayed.

11. Press `Enter` to finish the installation.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm