Open topic with navigation

# StartTimeout

The amount of time to wait to receive the first video frame from the XProtect recording server. If HPE Media Server does not receive video, the connection times out.

The value of this parameter is a time duration. Specify the duration in the following format:

Xminutes Yseconds

You can also shorten the string by abbreviating the units to their first letter (minutes abbreviates to n):

1n 3s

The following are all equivalent:

1minute 3seconds
1n 3s
63s

Type: | Time duration
Default: | 5 seconds
Required: | No
Configuration Section: | TaskName
Example: | `StartTimeout=3s`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm