Open topic with navigation

# Configure News Segmentation

To configure news segmentation , follow these steps.

To configure news segmentation

1. Create a new configuration to send to HPE Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Analysis]` section, add three analysis tasks. The first should run speech-to-text on an audio track of the ingested video. The second should run text segmentation to group the words extracted by speech-to-text into sentences. The third is the news segmentation task. For example:

       [Analysis]
       AnalysisEngine0=SpeechToText
       AnalysisEngine1=TextSegmentation
       AnalysisEngine2=NewsSegmentation

3. Create a new configuration section and configure the speech-to-text task. For information about how to set up speech-to-text, see Analyze Audio. For example:

       [SpeechToText]
       Type=SpeechToText
       Language=ENUS
       Mode=relative
       ModeValue=0.90
       FilterMusic=true

4. Create a new configuration section and configure the text segmentation task. For example:

       [TextSegmentation]
       Type=TextSegmentation
       Input=SpeechToText.Result

5. Create a new configuration section to contain the news segmentation task settings, and set the following parameters:

   `Type` | The analysis engine to use. Set this parameter to `NewsSegmentation`.
   `Input` | (Optional) The track to process. HPE recommends that you transcribe speech from the audio track of the news broadcast and then group the extracted words into sentences using a text segmentation task. Set this parameter to the result track of the text segmentation task.
   `IdolHost` | The host name or IP address of the IDOL Server (Content component) to use for news segmentation.
   `IdolPort` | The ACI port of the IDOL Server (Content component) to use for news segmentation.
   `MaxStoryDuration` | The maximum duration of a video segment that can be classified as a story. If a story exceeds this duration, Media Server begins a new story regardless of whether the concepts in the video have changed.

   For example:

       [NewsSegmentation]
       Type=NewsSegmentation
       Input=TextSegmentation.Result
       IdolHost=localhost
       IdolPort=9000
       MaxStoryDuration=30minutes

   For more information about the parameters that you can use to configure news segmentation, refer to the HPE Media Server Reference.

6. Save and close the configuration file. HPE recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm