Open topic with navigation

# NumParallel

The maximum number of video frames to analyze concurrently, where frames can be analyzed in parallel.

As long as your server has sufficient resources, increasing the value of this parameter allows HPE Media Server to analyze a greater number of frames in a given time. The result of this depends on the value you have set for IngestRate:

- If you are processing video with `IngestRate=1`, HPE Media Server is more likely to achieve the sample intervals that you have requested and your analysis tasks will skip fewer frames.
- If you are processing video with `IngestRate=0`, HPE Media Server can complete processing the video in less time.

Note: Do not increase the value of this parameter unless your server has spare resources (CPU cores), because doing so will significantly decrease performance.

This parameter has no effect on single images (HPE Media Server always uses a single thread on images).

Type: | Integer
Default: | 1
Required: | No
Configuration Section: | TaskName
Example: | To allow face demographics analysis to use up to two threads: `NumParallel=2`
See Also: | IngestRate

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm