Open topic with navigation

# MinRead

The minimum number of consecutive frames in which a plate must be visible before a result is returned, if the Integration parameter is set to `moving`.

In most cases HPE recommends that you use the default value. Reducing the value of this parameter could reduce accuracy.

Type: | Integer
Default: | 2
Required: | No
Configuration Section: | TaskName
Example: | `MinRead=5`
See Also: | Integration

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm