Open topic with navigation

# Example Barcode Task Configuration

To detect and read barcodes, you could use the following task configuration:

    [Barcodes]
    Type=barcode
    BarcodeTypes=all
    Orientation=any

Setting the `BarcodeTypes` parameter to `all` detects all types of barcodes, including QR codes.

By default HPE Media Server only detects barcodes that are upright, but setting the `Orientation` parameter to `any` means that HPE Media Server can also detect barcodes that have been rotated by 90 or 180 degrees.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm