Open topic with navigation

# Configure the Output Task

To configure an output task to insert information into a database, follow these steps.

To insert information into a database

1. Create a new configuration to send to HPE Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Output]` section, add a new output task by setting the `OutputEngineN` parameter. You can give the task any name, for example:

       [Output]
       OutputEngine0=MyDatabase

3. Below the `[Output]` section, create a configuration section for the engine by typing the task name inside square brackets. For example:

       [MyDatabase]

4. In the new section, set the following parameters:

   `Type` | The output engine to use. Set this parameter to `ODBC`.
   `Input` | (Optional) A comma-separated list of the tracks that contain information you want to output. Specify one or more tracks. If you do not set this parameter, the engine outputs all tracks that are configured by default as 'output' tracks. For information about whether a track is considered an 'output' track, refer to documentation for your analysis, encoding, and ESP engines in the HPE Media Server Reference.
   `OdbcConnectionString` | The ODBC connection string to use to connect to the database.
   `OdbcDriverManager` | (Linux only) The path of the ODBC driver manager shared library. This parameter is not required if you are running HPE Media Server on Windows.
   `XSLTemplate` | The path to the XSL template to use to extract values from records and construct a list of queries to run against the database.

5. Configure how to combine records into SQL queries. For more information about how you can combine records, see Choose How to Output Data.

   - To output data in single record mode, set `Mode=SingleRecord`.
   - To output data in time mode, set `Mode=Time` and use the `OutputInterval` parameter to specify the amount of video content represented by each document.
   - To output data in event mode, set `Mode=Event` and use the `EventTrack` parameter to specify the event track.
   - To output data in bounded event mode, set `Mode=BoundedEvent` and use the `EventTrack` parameter to specify the event track.
   - To output data in at-end mode, set `Mode=AtEnd`.
   - To output data in page mode, set `Mode=Page`.

6. Save and close the configuration file. HPE recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

Example

The following is an example configuration to output data using the ODBC output engine.

    [MyDatabase]
    Type=odbc
    OdbcConnectionString=DSN=MyDSN;
    Mode=singlerecord
    XslTemplate=./xsl/toODBC.xsl
    SavePreXML=true
    SavePostXML=true
    XMLOutputPath=./output/odbc/%segment.type%_%segment.sequence%.xml

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm