Open topic with navigation

# GetStreams

Returns a list of rolling buffers that have been configured.

Type: synchronous

## Example

    http://12.3.4.56:9000/action=GetStreams

This action uses port `9000` to contact HPE Media Server on a machine with the IP address `12.3.4.56`, to retrieve a list of rolling buffers.

## Response

A sample response appears below.

    <?xml version="1.0" encoding="UTF-8"?>
    <autnresponse xmlns:autn="http://schemas.autonomy.com/aci/">
    	<action>GETSTREAMS</action>
    	<response>SUCCESS</response>
    	<responsedata>
    		<stream>CCTV_cam1</stream>
    		<stream>CCTV_cam2</stream>
    	</responsedata>
    </autnresponse>

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm