Open topic with navigation

# AndAny Engine Configuration Parameters

An AndAny ESP task compares two tracks and produces a track containing records from the first track for which there is at least one event in the second track within a specified time interval (before or after the first track's event). This section describes the parameters that you can set in the configuration section for an AndAny ESP task.

Configuration Parameter | Description
--- | ---
Input0 | The first input track. A record from this track is added to the output if a record occurs in the second track within the specified time interval. If the LuaScript parameter is set your Lua function must also return `true`, otherwise the record is discarded.
Input1 | The second input track. Records from this track are never added to the output.
LuaScript | The path of a Lua script that contains a function to determine whether a record should be included in the output track.
MaxTimeInterval | The maximum interval from a record in the first track to a record in the second track, for the record in the first track to be included in the output.
MinTimeInterval | The minimum interval from a record in the first track to a record in the second track, for the record in the first track to be included in the output.
Type | The type of ESP engine to use. Set this parameter to `AndAny`.

## Output Tracks

This engine produces a single output track, named `TaskName.Output`. The output track has the same format as the input track Input0.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm