Open topic with navigation

# Transcribe Speech

To run speech-to-text

1. Create a new configuration to send to HPE Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Analysis]` section, add a new analysis task by setting the `AnalysisEngineN` parameter. You can give the task any name, for example:

       [Analysis]
       AnalysisEngine0=TranscribeSpeech

3. Create a new section to contain the settings for the task and set the following parameters:

   `Type` | The analysis engine to use. Set this parameter to `speechtotext`.
   `Input` | (Optional) The audio track to analyze. If you do not specify an input track, HPE Media Server processes the first track of the correct type produced by the ingest engine.
   `SpeechToTextServers` | The host name and ACI port of an IDOL Speech Server. Separate the host name and port with a colon (for example, `speechserver:15000`). You can specify multiple IDOL Speech Servers by using a comma-separated list. HPE Media Server can connect to only one IDOL Speech Server at a time, but you can provide multiple servers for failover. Tip: You can specify a default IDOL Speech Server to use for all speech-to-text tasks by setting the `SpeechToTextServers` parameter in the `[Resources]` section of the HPE Media Server configuration file.
   `Language` | The language pack to use. For a list of available language packs, refer to the IDOL Speech Server Administration Guide.
   `Mode` | The mode for speech-to-text transcription. HPE Media Server supports the following modes: `Fixed` `Relative` These modes are described in the IDOL Speech Server Reference.
   `ModeValue` | The mode value for speech-to-text transcription. For more information about this parameter, refer to the IDOL Speech Server Reference.
   `FilterMusic` | (Optional) Specifies whether to ignore speech-to-text results for audio segments that Speech Server identifies as music or noise. To filter these results from the output, set this parameter to `true`.
   `SampleFrequency` | (Optional) The sample frequency of the audio to send to the IDOL Speech Server for analysis, in samples per second (Hz). IDOL Speech Server language packs are dependent on the audio sample rate, and accept audio at either 8000Hz or 16000Hz.

   For example:

       [TranscribeSpeech]
       Type=speechtotext
       SpeechToTextServers=speechserver:13000
       Language=ENUK
       Mode=relative
       ModeValue=0.8
       FilterMusic=TRUE

   For more information about the parameters that you can use to configure speech-to-text, refer to the HPE Media Server Reference.

4. Save and close the configuration file. HPE recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm