Open topic with navigation

# Create a Configuration

To create a configuration, you need to consider:

- the media source, because this determines how to ingest the video.
- which analysis tasks you want to run, for example face recognition or speech-to-text.
- the way in which data will flow between tasks. For example, you cannot run face recognition without first running face detection. You must configure the input of the face recognition task to be the output from the face detection task.
- how to output data.

A HPE Media Server configuration can include `[Ingest]`, `[Analysis]`, `[Transform]`, `[Encoding]`, `[EventProcessing]`, and `[Output]` sections. Each section contains a list of tasks that you want to run:

    [Ingest]
    IngestEngine=LibAvIngest

    [Analysis]
    AnalysisEngine0=FaceDetect
    AnalysisEngine1=FaceRecognize
    ...

    [Transform]
    TransformEngine0=ResizeFaceImagesForEncoding
    ...

    [EventProcessing]
    EventProcessingEngine0=Deduplicate
    ...

    [Encoding]
    EncodingEngine0=Image
    ...

    [Output]
    OutputEngine0=IdolServer
    ...

These tasks are configured in other sections of the configuration file. The previous example defines an ingest task named `LibAvIngest` which you would configure in a section named `[LibAvIngest]`.

Every task configuration section contains the `Type` parameter to specify the engine to use to complete the task, and contains any settings that the engine requires to complete the task. For example:

    [LibAvIngest]
    Type=libav

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm