Open topic with navigation

# Format

The format of the video source.

In most cases HPE Media Server automatically detects the video format, but you must set this parameter to ingest raw video formats such as MJPEG, that have no container.

You can set this parameter to one of the following values:

- `avi`
- `asf`
- `flv`
- `gif`
- `h264`
- `hls`
- `mjpeg`
- `mpegts`

To ingest video from a video capture card that supports DirectShow, set this parameter to `dshow`. (You can use this value only on Windows platforms).

Type: | String
Default: |
Required: | No
Configuration Section: | TaskName
Example: | `Format=mpegts`
See Also: |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm