Open topic with navigation

# MaxRead

The maximum number of frames to use to read a single number plate.

- When the Integration parameter is set to `static`, ANPR does not return a result until it has received this number of frames.
- When the Integration parameter is set to `moving`, ANPR uses up to this number of frames to give one result.

Type: | Integer
Default: | 15
Allowed Range: | Maximum: 25
Required: | No
Configuration Section: | TaskName
Example: | `MaxRead=10`
See Also: | Integration

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm