Open topic with navigation

# Example Configuration

The following is an example configuration that runs news segmentation on ingested video. This configuration runs segmentation using an IDOL Server that is on the same machine as HPE Media Server. It also includes an output task to write the results of segmentation to files on disk.

    [Ingest]
    IngestEngine=libav

    [libav]
    Type=libav

    [Analysis]
    AnalysisEngine0=SpeechToText
    AnalysisEngine1=TextSegmentation
    AnalysisEngine2=NewsSegmentation

    [SpeechToText]
    Type=SpeechToText
    Language=ENUS
    Mode=relative
    ModeValue=0.90
    FilterMusic=true

    [TextSegmentation]
    Type=TextSegmentation
    Input=SpeechToText.Result

    [NewsSegmentation]
    Type=NewsSegmentation
    Input=TextSegmentation.Result
    IdolHost=localhost
    IdolPort=9000

    [Output]
    OutputEngine0=XML

    [XML]
    Type=xml
    Input=NewsSegmentation.Result,SpeechToText.Result
    Mode=bounded
    EventTrack=NewsSegmentation.Result
    XMLOutputPath=./output/%token%/Story_%segment.type%_%segment.sequence%.html

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm