Open topic with navigation

# IntervalsPerAsset

The number of output documents to index into an asset in Broadcast Monitoring. After this number of intervals, HPE Media Server starts a new asset.

For example, if you set `OutputInterval=30` and `IntervalsPerAsset=10`, HPE Media Server sends documents to Broadcast Monitoring that represent 30 seconds of video content. After 10 of these documents have been sent to Broadcast Monitoring and the asset represents 5 minutes of video, HPE Media Server starts a new asset.

You could set `OutputInterval=300` and `IntervalsPerAsset=1` to achieve the same result, but this would delay the indexing of data until HPE Media Server had processed 5 minutes of video content.

Type: | Integer
Default: | 1
Required: | No
Configuration Section: | TaskName
Example: | `IntervalsPerAsset=10`
See Also: | OutputInterval

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm