Open topic with navigation

# Milestone Ingest Engine Configuration Parameters

The Milestone ingest engine ingests live video from Milestone XProtect Enterprise or Milestone XProtect Corporate.

To configure an ingest task that uses the Milestone ingest engine, you can set the following parameters:

Configuration Parameter | Description
--- | ---
AuthenticationHost | The host name or IP address of the XProtect authentication server.
AuthenticationPort | The TCP port of the XProtect authentication server.
BasicPassword | A Milestone password to use to retrieve video. (Milestone XProtect Enterprise only).
BasicUserName | A Milestone user name to use to retrieve video. (Milestone XProtect Enterprise only).
NTLMPassword | An NT password to use to retrieve video.
NTLMUserName | An NT user name to use to retrieve video.
RecorderHost | The host name or IP address of the XProtect recording server.
RecorderPort | The TCP port of the XProtect recording server.
SOAPAuthentication | Specifies whether to authenticate against the XProtect authentication server instead of passing credentials to the XProtect recording server.
StartTimeout | The amount of time to wait to receive the first frame from the XProtect recording server.
Type | The type of ingest engine to use. Set this parameter to `MilestoneIngest`.

The Milestone ingest engine produces the following tracks:

- a proxy track, named `taskName.Proxy`, where `taskName` is the name of the ingest task.
- an image track, named `Image_1`.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm