Open topic with navigation

# Mode

Specifies how HPE Media Server combines information before creating queries to run against the database.

- `SingleRecord` - does not combine information. This mode creates one or more queries for every record. Use this mode when you want to insert data for discrete events, such as recognized number plates or words spoken in the audio.
- `Time` - each set of queries inserts data for the same amount of video content, for example 60 seconds of video. Specify the interval using the parameter OutputInterval. Each query can contain information from any records that relate to that time frame, including records that overlap the start or end of the interval. Each set of queries might insert data from many records, for example recognized faces, speech-to-text results, and on-screen text extracted using OCR.
- `Event` - use event mode to insert information for specific video segments, for example news stories in a news broadcast. HPE Media Server runs a separate set of queries for each record that occurs in an event track that you choose. Specify the event track using the parameter EventTrack. Each query can insert information about the event, from all records that overlap with that event, and all records that occurred since the end of the previous event. A pause in speech might indicate the end of one news story and the beginning of another, so you could configure HPE Media Server to create queries to insert the content between pauses in a speech-to-text result track.
- `Bounded` - use bounded mode to insert information about a specific event, for example a recognized speaker being detected in the audio track, and associated records that occurred during the same time. Specify the event track using the parameter EventTrack. In this mode, information cannot be output from a record unless it occurs at the same time as an event in the event track.
- `AtEnd` - use at-end mode to insert information about an asset, such as a video or image file. HPE Media Server runs one set of queries for each `process` action. The queries can contain information from the records that were generated when HPE Media Server processed that asset.
- `Page` - use page mode to insert information about a single page of a processed image or document.

Type: | String
Default: | Time
Required: | No
Configuration Section: | TaskName
Example: | `Mode=event`
See Also: | OutputInterval EventTrack

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm