Open topic with navigation

# Object Detection

Object Detection finds objects that belong to pre-defined classes, when they appear in media. For example, if you are processing video captured by a CCTV camera, you could train HPE Media Server to return the locations of pedestrians, cyclists, and cars that appear in the video.

Configuration Parameter | Description
--- | ---
DetectionThreshold | The minimum confidence score necessary for HPE Media Server to output an object detection result.
Detector | The detector to use for object detection.
Input | The track to analyze.
NumParallel | The maximum number of video frames to analyze simultaneously.
Region | The region of the frame to restrict processing to.
RegionUnit | The units to use when setting the Region parameter.
SampleInterval | The interval at which frames are selected to be analyzed, in milliseconds.
SyncDatabase | Specifies whether to synchronize with the training database before starting analysis.
Type | The analysis engine to use. Set this parameter to `ObjectDetection`.

## Output Tracks

Output track | Description
--- | ---
`Result` | HPE Media Server adds a record to this track for each object that is detected.
`ResultWithSource` | Records in this track contain the same data as those in the `Result` track, but also include the source image or video frame.

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm