Open topic with navigation

# Supported Barcode Types

HPE Media Server can read the following types of barcode:

Codabar | Data Matrix | Industrial 2/5 | UPC-A
Code-128 | EAN-13 | Matrix 2/5 | UPC-E
Code-39 | EAN-8 | Patch Code |
Code-93 | I25 | PDF417 |
Datalogic 2/5 | IATA 2/5 | QR |

© 2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm