Open topic with navigation

# Generate Diagnostics

The speech-to-text tasks can also generate diagnostic information. Generate diagnostic information before you contact customer support, to help them to solve issues more quickly.

To enable speech-to-text diagnostics

- Include the `Diag` and `DiagFile` parameters when you send the `AddTask` action. Set `Diag` to `True` and `DiagFile` to the name of the file to write the diagnostic information to.

For example:

    http://localhost:13000/action=AddTask&Type=WavToText&File=C:/myDataSpeech.wav&Out=SpeechTranscript.ctm&Lang=ENUS&Diag=True&DiagFile=Diagnostics.txt

This action uses port `13000` to instruct HPE IDOL Speech Server, which is located on the local machine, to perform the `WavToText` task on the `Speech.wav` file, and to write the results to the `SpeechTranscript.ctm` file and the diagnostics information to `Diagnostics.txt`.

© 2013-2016 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send Documentation Feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm